In [390]: runfile('/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany/main.py', wdir='/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany')

Reloaded modules: sim, config, components.socket, components.battery, components.ev, components.bss, components.pv_surplus_handler, data_manager, statistics_GC, plot

PV: 0 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 101.114842

Mean net cost: 101.114842

Max PV stored energy: 0.000000

Cost per service: 0.993457

Mean consumption: 1609649.748941

Mean grid consumption: 1609649.748941

Mean SPV: 0.000000

Mean saving: 0.000000

-

PV: 300 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 64.979983

Mean net cost: 59.610622

Max PV stored energy: 85.903212

Cost per service: 0.638431

Mean consumption: 1609649.748941

Mean grid consumption: 1020669.920874

Mean SPV: 588979.828067

Mean saving: 5.369361

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 55.997661

Mean net cost: 41.637631

Max PV stored energy: 143.439802

Cost per service: 0.550179

Mean consumption: 1609649.748941

Mean grid consumption: 880176.058732

Mean SPV: 729473.690209

Mean saving: 14.360030

-

PV: 700 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 51.514815

Mean net cost: 26.274940

Max PV stored energy: 76.309364

Cost per service: 0.506135

Mean consumption: 1609649.748941

Mean grid consumption: 811526.626962

Mean SPV: 798123.121979

Mean saving: 25.239875

-

PV: 900 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 48.898339

Mean net cost: 11.932304

Max PV stored energy: 131.806601

Cost per service: 0.480428

Mean consumption: 1609649.748941

Mean grid consumption: 771638.675785

Mean SPV: 838011.073156

Mean saving: 36.966035

-

PV: 1100 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 47.191835

Mean net cost: -1.636175

Max PV stored energy: 2.305976

Cost per service: 0.463661

Mean consumption: 1609649.748941

Mean grid consumption: 745744.082190

Mean SPV: 863905.666750

Mean saving: 48.828011

-

PV: 1300 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 45.983760

Mean net cost: -15.059457

Max PV stored energy: 55.321703

Cost per service: 0.451792

Mean consumption: 1609649.748941

Mean grid consumption: 727476.058776

Mean SPV: 882173.690165

Mean saving: 61.043217

-

PV: 1500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 45.078888

Mean net cost: -28.332508

Max PV stored energy: 5.688143

Cost per service: 0.442902

Mean consumption: 1609649.748941

Mean grid consumption: 713818.496591

Mean SPV: 895831.252349

Mean saving: 73.411396

-

ok?

ok?

In [391]: