In [359]: runfile('/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany/main.py', wdir='/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany')

Reloaded modules: sim, config, components.socket, components.battery, components.ev, components.bss, components.pv_surplus_handler, data_manager, statistics_GC, plot

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 0 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 55.997661

Mean net cost: 41.637631

Max PV stored energy: 143.439802

Cost per service: 0.550179

Mean consumption: 1609649.748941

Mean grid consumption: 880176.058732

Mean SPV: 729473.690209

Mean saving: 14.360030

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 10 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 1.301370

Mean cost: 51.073064

Mean net cost: 38.043976

Max PV stored energy: 0.000000

Cost per service: 0.508169

Mean consumption: 1573786.573577

Mean grid consumption: 823444.493810

Mean SPV: 750342.079767

Mean saving: 13.029089

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 11 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 1.706849

Mean cost: 50.218228

Mean net cost: 37.234799

Max PV stored energy: 0.000000

Cost per service: 0.501687

Mean consumption: 1565966.525467

Mean grid consumption: 813279.935700

Mean SPV: 752686.589767

Mean saving: 12.983429

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 12 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 2.134247

Mean cost: 49.317508

Mean net cost: 36.387900

Max PV stored energy: 0.000000

Cost per service: 0.494802

Mean consumption: 1557189.670855

Mean grid consumption: 802248.787837

Mean SPV: 754940.883018

Mean saving: 12.929608

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 13 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 2.728767

Mean cost: 48.200047

Mean net cost: 35.325304

Max PV stored energy: 0.000000

Cost per service: 0.486492

Mean consumption: 1545472.266283

Mean grid consumption: 787754.774156

Mean SPV: 757717.492127

Mean saving: 12.874743

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 14 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 3.457534

Mean cost: 46.914843

Mean net cost: 34.107283

Max PV stored energy: 0.000000

Cost per service: 0.477029

Mean consumption: 1530032.698100

Mean grid consumption: 769922.594547

Mean SPV: 760110.103553

Mean saving: 12.807560

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 15 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 4.391781

Mean cost: 45.334482

Mean net cost: 32.521812

Max PV stored energy: 0.000000

Cost per service: 0.465381

Mean consumption: 1509483.659578

Mean grid consumption: 747115.813331

Mean SPV: 762367.846247

Mean saving: 12.812669

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 16 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 5.761644

Mean cost: 43.475685

Mean net cost: 30.762517

Max PV stored energy: 0.000000

Cost per service: 0.452665

Mean consumption: 1482374.806929

Mean grid consumption: 718609.530758

Mean SPV: 763765.276172

Mean saving: 12.713168

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 7.539726

Mean cost: 41.297572

Mean net cost: 28.611712

Max PV stored energy: 0.000000

Cost per service: 0.438097

Mean consumption: 1448654.851152

Mean grid consumption: 683618.626912

Mean SPV: 765036.224241

Mean saving: 12.685860

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 18 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 10.054795

Mean cost: 38.737959

Mean net cost: 26.062808

Max PV stored energy: 0.000000

Cost per service: 0.422209

Mean consumption: 1406647.683716

Mean grid consumption: 641379.113436

Mean SPV: 765268.570281

Mean saving: 12.675151

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 19 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 13.315068

Mean cost: 35.922569

Mean net cost: 23.280315

Max PV stored energy: 0.000000

Cost per service: 0.405949

Mean consumption: 1358476.753750

Mean grid consumption: 593568.277687

Mean SPV: 764908.476063

Mean saving: 12.642254

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 20 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 17.712329

Mean cost: 32.972997

Mean net cost: 20.402158

Max PV stored energy: 0.000000

Cost per service: 0.392101

Mean consumption: 1306563.431186

Mean grid consumption: 542281.200047

Mean SPV: 764282.231139

Mean saving: 12.570840

-

[0, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20]

[0, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20]

In [360]: