In [367]: runfile('/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany/main.py', wdir='/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany')

Reloaded modules: sim, config, components.socket, components.battery, components.ev, components.bss, components.pv_surplus_handler, data_manager, statistics_GC, plot

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 55.997661

Mean net cost: 41.637631

Max PV stored energy: 143.439802

Cost per service: 0.550179

Mean consumption: 1609649.748941

Mean grid consumption: 880176.058732

Mean SPV: 729473.690209

Mean saving: 14.360030

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 60

Mean arrivals: 101.805479

Mean loss: 4.027397

Mean cost: 49.309772

Mean net cost: 35.571567

Max PV stored energy: 0.000000

Cost per service: 0.504303

Mean consumption: 1553539.595533

Mean grid consumption: 822710.409174

Mean SPV: 730829.186359

Mean saving: 13.738205

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 120

Mean arrivals: 101.805479

Mean loss: 4.830137

Mean cost: 47.404754

Mean net cost: 33.916140

Max PV stored energy: 0.000000

Cost per service: 0.488833

Mean consumption: 1531775.720691

Mean grid consumption: 797862.170589

Mean SPV: 733913.550102

Mean saving: 13.488614

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 180

Mean arrivals: 101.805479

Mean loss: 5.194521

Mean cost: 46.811699

Mean net cost: 33.490755

Max PV stored energy: 0.000000

Cost per service: 0.484538

Mean consumption: 1522244.517528

Mean grid consumption: 786366.596083

Mean SPV: 735877.921445

Mean saving: 13.320944

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 240

Mean arrivals: 101.805479

Mean loss: 5.443836

Mean cost: 46.294071

Mean net cost: 33.056827

Max PV stored energy: 0.000000

Cost per service: 0.480420

Mean consumption: 1513120.924236

Mean grid consumption: 775357.384313

Mean SPV: 737763.539923

Mean saving: 13.237245

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 300

Mean arrivals: 101.805479

Mean loss: 5.810959

Mean cost: 45.480881

Mean net cost: 32.310865

Max PV stored energy: 143.439802

Cost per service: 0.473786

Mean consumption: 1499982.214609

Mean grid consumption: 758299.749807

Mean SPV: 741682.464803

Mean saving: 13.170016

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 360

Mean arrivals: 101.805479

Mean loss: 6.358904

Mean cost: 44.190617

Mean net cost: 31.198764

Max PV stored energy: 143.439802

Cost per service: 0.462988

Mean consumption: 1481815.179203

Mean grid consumption: 732749.582068

Mean SPV: 749065.597135

Mean saving: 12.991853

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 420

Mean arrivals: 101.805479

Mean loss: 6.893151

Mean cost: 42.790314

Mean net cost: 29.939523

Max PV stored energy: 143.439802

Cost per service: 0.450840

Mean consumption: 1461972.055290

Mean grid consumption: 706979.347823

Mean SPV: 754992.707467

Mean saving: 12.850790

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 7.539726

Mean cost: 41.297572

Mean net cost: 28.611712

Max PV stored energy: 0.000000

Cost per service: 0.438097

Mean consumption: 1448654.851152

Mean grid consumption: 683618.626912

Mean SPV: 765036.224241

Mean saving: 12.685860

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 540

Mean arrivals: 101.805479

Mean loss: 7.597260

Mean cost: 40.979778

Mean net cost: 28.463209

Max PV stored energy: 0.000000

Cost per service: 0.434992

Mean consumption: 1445065.249744

Mean grid consumption: 680196.515776

Mean SPV: 764868.733968

Mean saving: 12.516569

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 600

Mean arrivals: 101.805479

Mean loss: 7.616438

Mean cost: 41.028045

Mean net cost: 28.487045

Max PV stored energy: 0.000000

Cost per service: 0.435593

Mean consumption: 1441534.633116

Mean grid consumption: 677650.531048

Mean SPV: 763884.102068

Mean saving: 12.541000

-

[0, 60, 120, 180, 240, 300, 360, 420, 480, 540, 600]

[0, 60, 120, 180, 240, 300, 360, 420, 480, 540, 600]

In [368]: