In [364]: runfile('/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany/main.py', wdir='/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany')

Reloaded modules: sim, config, components.socket, components.battery, components.ev, components.bss, components.pv_surplus_handler, data_manager, statistics_GC, plot

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 55.997661

Mean net cost: 41.637631

Max PV stored energy: 143.439802

Cost per service: 0.550179

Mean consumption: 1609649.748941

Mean grid consumption: 880176.058732

Mean SPV: 729473.690209

Mean saving: 14.360030

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 60

Mean arrivals: 101.805479

Mean loss: 4.032877

Mean cost: 49.238728

Mean net cost: 35.316747

Max PV stored energy: 0.000000

Cost per service: 0.503605

Mean consumption: 1554611.775092

Mean grid consumption: 825148.971030

Mean SPV: 729462.804061

Mean saving: 13.921981

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 120

Mean arrivals: 101.805479

Mean loss: 4.734247

Mean cost: 47.416201

Mean net cost: 33.479674

Max PV stored energy: 0.000000

Cost per service: 0.488468

Mean consumption: 1536564.460911

Mean grid consumption: 806090.262826

Mean SPV: 730474.198085

Mean saving: 13.936527

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 180

Mean arrivals: 101.805479

Mean loss: 5.063014

Mean cost: 46.425456

Mean net cost: 32.393500

Max PV stored energy: 0.000000

Cost per service: 0.479887

Mean consumption: 1530572.519020

Mean grid consumption: 794370.041404

Mean SPV: 736202.477616

Mean saving: 14.031957

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 240

Mean arrivals: 101.805479

Mean loss: 5.509589

Mean cost: 44.689162

Mean net cost: 31.034757

Max PV stored energy: 0.000000

Cost per service: 0.464082

Mean consumption: 1518070.505521

Mean grid consumption: 772046.574252

Mean SPV: 746023.931269

Mean saving: 13.654405

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 300

Mean arrivals: 101.805479

Mean loss: 5.709589

Mean cost: 43.779591

Mean net cost: 30.096984

Max PV stored energy: 91.324353

Cost per service: 0.455582

Mean consumption: 1511129.598770

Mean grid consumption: 759196.778023

Mean SPV: 751932.820747

Mean saving: 13.682608

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 360

Mean arrivals: 101.805479

Mean loss: 5.879452

Mean cost: 42.964119

Mean net cost: 29.444581

Max PV stored energy: 91.324353

Cost per service: 0.447888

Mean consumption: 1502038.391878

Mean grid consumption: 746697.776148

Mean SPV: 755340.615730

Mean saving: 13.519538

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 420

Mean arrivals: 101.805479

Mean loss: 5.882192

Mean cost: 42.829574

Mean net cost: 29.311162

Max PV stored energy: 91.324353

Cost per service: 0.446498

Mean consumption: 1501345.729776

Mean grid consumption: 746326.418299

Mean SPV: 755019.311477

Mean saving: 13.518412

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 5.909589

Mean cost: 42.704014

Mean net cost: 29.157017

Max PV stored energy: 91.324353

Cost per service: 0.445316

Mean consumption: 1501250.381678

Mean grid consumption: 745575.173113

Mean SPV: 755675.208564

Mean saving: 13.546997

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 540

Mean arrivals: 101.805479

Mean loss: 5.945205

Mean cost: 42.666984

Mean net cost: 29.137865

Max PV stored energy: 91.324353

Cost per service: 0.445096

Mean consumption: 1500897.966903

Mean grid consumption: 745218.054098

Mean SPV: 755679.912805

Mean saving: 13.529120

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 600

Mean arrivals: 101.805479

Mean loss: 5.947945

Mean cost: 42.670282

Mean net cost: 29.141055

Max PV stored energy: 91.324353

Cost per service: 0.445143

Mean consumption: 1501033.595757

Mean grid consumption: 745358.387193

Mean SPV: 755675.208564

Mean saving: 13.529227

-

[0, 60, 120, 180, 240, 300, 360, 420, 480, 540, 600]

[0, 60, 120, 180, 240, 300, 360, 420, 480, 540, 600]

In [365]: