In [362]: runfile('/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany/main.py', wdir='/home/daniela/Documents/politecnico/research_activity/research_topics/Battery_Switching_Stations/BSS-main_Dany')

Reloaded modules: sim, config, components.socket, components.battery, components.ev, components.bss, components.pv_surplus_handler, data_manager, statistics_GC, plot

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 0

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 55.997661

Mean net cost: 41.637631

Max PV stored energy: 143.439802

Cost per service: 0.550179

Mean consumption: 1609649.748941

Mean grid consumption: 880176.058732

Mean SPV: 729473.690209

Mean saving: 14.360030

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 60

Mean arrivals: 101.805479

Mean loss: 0.024658

Mean cost: 55.968226

Mean net cost: 41.608438

Max PV stored energy: 143.439802

Cost per service: 0.549890

Mean consumption: 1608101.920490

Mean grid consumption: 878620.245359

Mean SPV: 729481.675132

Mean saving: 14.359789

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 120

Mean arrivals: 101.805479

Mean loss: 0.054795

Mean cost: 55.751244

Mean net cost: 41.438401

Max PV stored energy: 143.439802

Cost per service: 0.547920

Mean consumption: 1603780.309857

Mean grid consumption: 872935.321987

Mean SPV: 730844.987869

Mean saving: 14.312843

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 180

Mean arrivals: 101.805479

Mean loss: 0.123288

Mean cost: 55.189731

Mean net cost: 41.219045

Max PV stored energy: 143.439802

Cost per service: 0.542767

Mean consumption: 1598476.109185

Mean grid consumption: 861956.441203

Mean SPV: 736519.667982

Mean saving: 13.970686

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 240

Mean arrivals: 101.805479

Mean loss: 0.315068

Mean cost: 54.152422

Mean net cost: 40.614929

Max PV stored energy: 143.439802

Cost per service: 0.533572

Mean consumption: 1591006.534418

Mean grid consumption: 843874.845078

Mean SPV: 747131.689340

Mean saving: 13.537493

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 300

Mean arrivals: 101.805479

Mean loss: 0.575342

Mean cost: 53.027686

Mean net cost: 39.948469

Max PV stored energy: 0.000000

Cost per service: 0.523833

Mean consumption: 1580714.102725

Mean grid consumption: 824350.035397

Mean SPV: 756364.067328

Mean saving: 13.079216

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 360

Mean arrivals: 101.805479

Mean loss: 0.849315

Mean cost: 51.986769

Mean net cost: 39.210731

Max PV stored energy: 688.146661

Cost per service: 0.514944

Mean consumption: 1567056.398998

Mean grid consumption: 806244.688504

Mean SPV: 760811.710495

Mean saving: 12.776038

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 420

Mean arrivals: 101.805479

Mean loss: 1.180822

Mean cost: 50.880867

Mean net cost: 37.764529

Max PV stored energy: 586.396318

Cost per service: 0.505650

Mean consumption: 1547302.926481

Mean grid consumption: 787106.659795

Mean SPV: 760196.266686

Mean saving: 13.116337

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 480

Mean arrivals: 101.805479

Mean loss: 1.643836

Mean cost: 49.754262

Mean net cost: 36.792191

Max PV stored energy: 18.983529

Cost per service: 0.496740

Mean consumption: 1524107.990230

Mean grid consumption: 768745.508572

Mean SPV: 755362.481658

Mean saving: 12.962071

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 540

Mean arrivals: 101.805479

Mean loss: 2.854795

Mean cost: 48.390154

Mean net cost: 35.421743

Max PV stored energy: 143.439802

Cost per service: 0.489033

Mean consumption: 1496182.677751

Mean grid consumption: 749946.168916

Mean SPV: 746236.508834

Mean saving: 12.968411

-

PV: 500 , NBSS: 20 , BTH: 18000.0 , WMAX: 15 , F: 17 , TMAX: 600

Mean arrivals: 101.805479

Mean loss: 3.638356

Mean cost: 47.720729

Mean net cost: 34.383768

Max PV stored energy: 143.439802

Cost per service: 0.486117

Mean consumption: 1480328.542856

Mean grid consumption: 737736.747752

Mean SPV: 742591.795105

Mean saving: 13.336961

-

[0, 60, 120, 180, 240, 300, 360, 420, 480, 540, 600]

[0, 60, 120, 180, 240, 300, 360, 420, 480, 540, 600]

In [363]: