
@Article{su11247096,
AUTHOR = {Kim, Ho-Jeong and Yang, Chang-Seok and Moon, Hyeun Jun},
TITLE = {A Study on Multi-Objective Parametric Design Tool for Surround-Type Movable Shading Device},
JOURNAL = {Sustainability},
VOLUME = {11},
YEAR = {2019},
NUMBER = {24},
ARTICLE-NUMBER = {7096},
URL = {https://www.mdpi.com/2071-1050/11/24/7096},
ISSN = {2071-1050},
ABSTRACT = {This study presents a multi-objective parametric design tool for four-axis surround-type movable shading device using solar position tracking in Seoul, South Korea. In order to explore large numbers of possible forms of shades, generic algorithms are utilized with real-time simulation of the performative criteria such as solar radiation, daylight glare probability (DGP), and solar shielding rate on window surface. This study outlines a workflow using a multi-objective engine called Octopus that runs within Grasshopper 3D, a parametric design tool, in addition to environmental performance simulation plug-in Ladybug. The workflow utilizes a performance-based design tool, which allows the designer to explore, sort, and filter solutions, and visually compare alternative solutions in terms of energy saving and indoor daylight quality in order to determine the optimal form of shade changing its shape every one hour. The result of deriving and analyzing the optimal shade shape through the genetic algorithm proposed in this study is as follows: On the one hand, on the summer solstice, shade shapes with shielding areas of almost 100% should be derived to achieve the most effective reduction of the direct solar radiation. The proposed movable shading device reduced direct solar radiation by 52.40% and 57.20% in the south- and east-facing windows, respectively. On the other hand, in winter when solar heat gain is important, the absence of sunshade is optimal in terms of heating load. However, in order to improve the indoor light environment, it is confirmed that it is possible to derive a certain shape of sunshade according to the sun&rsquo;s trajectory. On the winter solstice, the problem of glare arises from 10:00 to 15:00 in the south and 10:00 in the east. Therefore, the proposed four-axis movable shading device can be configured to have a minimum protrusion length satisfying DGP less than 0.35 in winter.},
DOI = {10.3390/su11247096}
}



