# To measure air quality

LogicalFunction

Test3 > Test3 > Logical Architecture > Logical Functions > Root Logical Function > To test ECLS technologies > To monitor atmosphere system > To measure air quality

No description.

## Involving Functional Chains

- Atmosphere Functional Chain

## Allocating Component

- Atmosphere Control and Monitoring

## Incoming Functional Ports

- FIP 1

## Outgoing Functional Ports

- FOP 1
- FOP 2

## Incoming Functional Exchanges

Exchange | Involving functional chains | Allocating component Exchanges | Distant Port | Source | Description | Allocated Exchange Items | Realized Functional Exchange | Realizing Functional Exchange
--- | --- | --- | --- | --- | --- | --- | --- | ---
Quality monitoring | Atmosphere Functional Chain |  | FOP 1 | Gather 14 |  |  |  |

## Outgoing Functional Exchanges

Exchange | Involving functional chains | Allocating component Exchanges | Distant Port | Target | Description | Allocated Exchange Items | Realized Functional Exchange | Realizing Functional Exchange
--- | --- | --- | --- | --- | --- | --- | --- | ---
Checking results | Atmosphere Functional Chain |  | FIP 1 | Split 18 |  |  |  |
Transferring data | Atmosphere Functional Chain |  | FIP 10 | To manage data |  |  |  |

## Diagrams displaying "To measure air quality"

- [ES] ECLS Technologies Logical Scenario
- [LAB] ECLS Technologies Structure
- [LFBD] ECLS Technologies Root Logical Function