# To measure atmospheric conditions

LogicalFunction

Test3 > Test3 > Logical Architecture > Logical Functions > Root Logical Function > To test human environment interactions > To monitor environmental parameters > To measure atmospheric conditions

No description.

## Involving Functional Chains

- Environment Functional Chain

## Allocating Component

- Atmosphere Control and Monitoring

## Outgoing Functional Ports

- FOP 1

## Outgoing Functional Exchanges

Exchange | Involving functional chains | Allocating component Exchanges | Distant Port | Target | Description | Allocated Exchange Items | Realized Functional Exchange | Realizing Functional Exchange
--- | --- | --- | --- | --- | --- | --- | --- | ---
Chechking results | Environment Functional Chain |  | FIP 1 | Duplicate 23 |  |  |  |

## Diagrams displaying "To measure atmospheric conditions"

- [ES] Human Environment Interactions Logical Scenario
- [LAB] Human Environment Interactions and Crew Support Facilities Structure
- [LFBD] Human Environment Interactions and Crew Support Facilities Root Logical Function